
**Project Title:** Atomistic Modeling of Thermal Transport in Large Unit Cell Crystals for Thermoelectric Energy Generation

**Research Team:**

Graduate Student: Jason Larkin, Mechanical Engineering  
Faculty Advisor: Associate Professor Alan McGaughey, Mechanical Engineering  
Affiliated Faculty: Visiting Professor Wissam Al-Saidi, Department of Chemical and Petroleum Engineering, University of Pittsburgh

**Project Description**

*The objective of this project is to build a robust, accurate, and efficient computational framework for predicting the thermal conductivity of large unit cell crystalline solids for improving the efficiency of thermoelectric energy generation.*


Thermoelectric energy generation - the transformation of waste heat into useful electricity - is a promising source of sustainable energy [cite]. Thermoelectric materials directly convert temperature differences into electric voltage as a result of their intrinsic (atomic-level) electronic and thermal properties. The performance of a thermoelectric device can be quantified through the *thermoelectric figure of merit*, ***ZT* =** , where *T* is the average device temperature, *S* is the Seebeck coefficient (the ratio of the induced thermoelectric voltage to the applied temperature difference), is the electrical conductivity, and is the *thermal conductivity*. For thermoelectric devices to be competitive with traditional power generation cycles requires *ZT* > 3 [Chen]. Achieving this performance is challenging because the electrical and thermal properties in *ZT* are coupled in the majority of materials [Chen, Dresselhaus]. The ideal thermoelectric can be thought of as an “electron-crystal/ phonon-glass” (high , low ) (see Figure 1). Reducing has become a primary strategy in the design of new thermoelectric materials [Dresselhaus]. Using nanostructuring to reduce while maintaining good electrical properties has been identified as one possible strategy [Minnich], but such materials are costly. An emerging area of study is the use of large unit cell (LUC) crystals [Dresselhaus].

Figure 1: LUC crystals can maximize *ZT*. ZT.

Large unit cell crystals have an ordered (crystalline) structure, but the basic building block (unit cell) of the crystal has a large number of distinct atoms (Figure 1) [Skutt, Yang1, Yang2]. They are thus effectively disordered over length scales on the order of the atomic spacing and their thermal conductivities can be as low as a glass [Skutt, Zintl, Yang1, Yang2]. The key advantage of LUC materials is that they are still ordered from the standpoint of electrons, which results in large and *ZT*. Thus, LUC crystals are “electron-crystal/phonon-glass” Materials. Current LUC crystals have *ZT*<3 [Skutt, Zintl] and more research is required to improve their thermoelectric performance.

The LUC crystals to be studied here are skutterudites [Skutt] and Zintl compounds [Zintl] (Figure 2). Both of these LUC crystals have [Skutt, Zintl], but experimental measurements show intriguing potential for improved thermoelectric efficiency [Yang1, Yang2]. Identifying design strategies for improving skutterudite and Zintl compound *ZT* requires detailed atomistic analyses. The necessary computational tools and resources are available in my research group, the Nanoscale Transport Phenomena Laboratory (NTPL), [Larkin, ALD1, ALD2]. Classical simulations will be used in preliminary testing to study the structural features of LUC crystals that lead to low (*Objective 1*) [Larkin,ALD1, ALD2]. These medium-accuracy classical simulation results will then be used to design computationally-intensive *ab initio* (quantum mechanical) simulations, which have high accuracy (*Objective 2*) [DFPT]. From these *ab initio* simulations, structural features that lead to low will be identified with high accuracy to improve *ZT*. The *ab initio* simulation results will be validated against limited experimental data [Skutt,Zintl, Yang1, Yang2], and used to provide guidance to the experimental community working on these exciting materials (*Objective 3*).

The use of *ab initio* calculations to inform the design of materials with desired thermal properties is an emerging field. The ability for the team to attract external funding will be greatly improved through the Dowd Fellowship, which will enable demonstration of the validity of the approach and generate important preliminary data,

****

**Research Plan**

Figure 2: Large unit cell skutterudite compound [cite].

***Objective 1****: Use classical molecular and lattice dynamics calculations to explore LUC crystal design concepts.*

As the name suggests, LUC materials require a large number of atoms to model accurately [Skutt,Zintl]. Size effects will be tested to ensure converged results, as in [Galli]. Classical simulations are time-efficient, so they are ideal for preliminary testing. These simulations will be conducted to explore structural features that lead to low . For example, the influence of “rattler” atom mass and bonding on reducing will be explored (Figure 2) [Yang1, Yang2]. The results will identify important trends in structural properties that reduce , which will be valuable when designing time-efficient *ab initio* simulations.

***Objective 2:*** *Design ab initio simulations to predict the thermal properties of realistic LUC crystals.*

*Ab initio* simulations have high accuracy, but are very computationally expensive. The classical simulation results from *Objective 1* will be used to design time-efficient *ab initio* simulations. Simulations of sutterudites and Zintl compounds will be run on the extensive resources NTPL has at the Engineer Research and Development Center (ERDC) [DFPT]. The structural features that reduce (from *Objective 1*) will be identified with higher accuracy to allow for direct comparison with available experimental data.

***Objective 3:*** *Report ab-initio simulation results to publishing journal(s) and experiments to improve ZT over existing LUC materials.*

These above objectives can be used iteratively, with data from real experiments, to efficiently search the large unit cell design space. ***Ab-initio simulations can predict large unit cell materials with even lower thermal conductivities, and thus increase ZT>3.***

**Relationship to CIT/ICES Strategic Focus**

Atomistic simulation of LUC materials fits directly into CIT’s nanotechnology initiative. This project is aligned with ICES’s Center for Multiscale Modeling for Engineering Materials (CM2EM) and Center for Nano-enabled Device and Energy Technologies (CNXT), both of which McGaughey is affiliated with. The work provides a compelling example of multi-scale and multi-physics modeling by demonstrating how classical-level (molecular and lattice dynamics) simulations can inform quantum-level (ab-initio) simulations, maximizing the impact of both.

**Present and Future Funding**

Preliminary funding for Larkin’s research has been through a CIT Dean’s fellowship, funds from the Department of Mechanical Engineering, and extra funds from an AFOSR project. He does not have support in place for the 2011-2012 academic year.

The Dowd fellowship will enable the team to initiate first-principles study of thermal transport in LUC materials. With critical preliminary data in hand, the team will be competitive for funding from NSF’s Thermal Transport Processes (ENG-CBET) and Condensed Matter and Materials Theory (DMR) programs and DOE’s Condensed Matter and Materials Physics (BES-MSE) and Computational and Theoretical Chemistry (BES-CSGB) programs. In the future, the team will seek out experimental collaborators in materials synthesis and thermal measurements [notably Jon Malen (ME), who thermally characterizes micro- and nanoscale materials and currently collaborates with McGaughey on other projects]. Together, they will apply for funding from NSF’s Interdisciplinary Research (IDR) program.

**References**

[Larkin] J. Larkin, A. J. H. McGaughey, “Predicting Phonon Properties of Defected Systems using Spectral Energy Density”, in preparation.

[Galli] Y. He, D. Donadio, G. Galli, “Heat Transport in Amorphous Silicon: Interplay between morphology and disorder”, Appl. Phys. Lett. 98 (2011) 144101.

[Skutt] T. He, J. Chen, H. D. Rosenfeld, M. A. Subramanian, “Thermoelectric Properties of Indium-Filled Skutterudites”, Chem. Mater., 2006, 18 (3), pp 759–762.

[Zintl] X.-J. Wang, M.-B. Tang, J.-T. Zhao, H.-H. Chen, X.-X. Yang, “Thermoelectric properties and electronic structure of Zintl compound BaZn2Sb2”, Appl. Phys. Lett. 90, 232107 (2007).

[Yang1] Yang, et al., “Effect of La filling on thermoelectric properties of LaxCo3.6Ni0.4Sb12-filled skutterudite prepared by MA-HP method”, Journal of Solid State Chemistry 179 (2006) 212-216.

[Yang2] Pend, et al., “Effect of Fe substitution on the thermoelectric transport properties of CoSb3-based Skutterudite compound”, Journal of Alloys and Compounds 426 (2006) 7-11.

[Chen] G. Chen, M. S. Dresselhaus, G. Dresselhaus, J.-P. Fleurial, and T. Caillat, “Recent developments in thermoelectric materials.” *International Materials Reviews* **48** (2003) 45–66.

[Dresselhaus] M.S. Dresselhaus, et al., “New Directions for Low-Dimensional Thermoelectric Materials”, Adv. Mater. 2007, 19, 1043–1053.

[Minnich] A. J. Minnich, M. S. Dresselhaus, F. Ren, and G. Chen, “Bulk nanostructured thermoelectric materials: current research and future prospects”, *Energy and Environmental Sciences* **2** (2009) 466–479.

[DFPT] S. Baroni, S. de Gironcoli, A. Dal Corso, and P. Giannozzi, “Phonons and related crystal

properties from density-functional perturbation theory.” *Reviews of Modern Physics* **73** (2001)

515–562.

[ALD1] J. E. Turney, E. S. Landry, A. J. H. McGaughey, and C. H. Amon, “Predicting phonon properties and thermal conductivity from anharmonic lattice dynamics calculations and molecular dynamics simulations.” *Physical Review B* **79** (2009) 064301.

[ALD2] S. Shenogin, A. Bodapati, P. Keblinski, and A. J. H. McGaughey, “Predicting the thermal conductivity of inorganic and polymeric glasses: The role of anharmonicity.” *Journal of Applied* *Physics* **105** (2009) 034906.

[1] N. W. Ashcroft and N. D. Mermin, *Solid State Physics*. Saunders, Fort Worth (1976).

[11] G. J. Snyder and E. S. Toberer, “Complex thermoelectric materials.” *Nature Materials* **7** (2008)

105–114.

[20] P. K. Schelling, S. R. Phillpot, and P. Keblinski, “Comparison of atomic-level simulation

methods for computing thermal conductivity.” *Physical Review B* **65** (2002) 144306.

[21] A. J. H. McGaughey and M. Kaviany, “Quantitative validation of the Boltzmann transport

equation phonon thermal conductivity model under the single-mode relaxation time approximation.” *Physical Review B* **69** (2004) 094303.

[22] A. J. H. McGaughey and M. Kaviany, “Phonon transport in molecular dynamics simulations: Formulation and thermal conductivity prediction.” In G. A. Greene, Y. I. Cho, J. P. Hartnett,

and A. Bar-Cohen (eds.), “Advances in Heat Transfer, Volume 39,” Elsevier (2006) 169–255.

[23] D. P. Sellan, E. S. Landry, J. E. Turney, A. J. H. McGaughey, and C. H. Amon, “Size effects in

molecular dynamics thermal conductivity predictions.” *Physical Review B* **81** (2010) 214305.

[30] D. A. Broido, M. Maloney, G. Birner, N. Mingo, and D. Stewart, “Intrinsic lattice thermal conductivity

of semiconductors from first principles.” *Applied Physics Letters* **91** (2007) 231922.

[31] K. Esfarjani and H. T. Stokes, “Method to extract anharmonic force constants from first principles calculations.” *Physical Review B* **77** (2008) 144112.

[33] J. E. Turney, A. J. H. McGaughey, and C. H. Amon, “Assessing the applicability of quantum corrections to classical thermal conductivity predictions.” *Physical Review B* **79** (2009) 224305.

[34] J. E. Turney, A. J. H. McGaughey, and C. H. Amon, “In-plane phonon transport in thin films.”

*Journal of Applied Physics* **107** (2010) 024317.

[35] A. J. C. Ladd, B. Moran, and W. G. Hoover, “Lattice thermal conductivity: A comparison

of molecular dynamics and anharmonic lattice dynamics.” *Physical Review B* **34** (1986) 5058–

5064.

[36] A. J. H. McGaughey, M. I. Hussein, E. S. Landry, M. Kaviany, and G. M. Hulbert, “Phonon

band structure and thermal transport correlation in a layered diatomic crystal.” *Physical*

*Review B* **74** (2006) 104304.

[37] A.Ward, D. A. Broido, D. A. Stewart, and G. Deinzer, “Ab initio theory of the lattice thermal

conductivity in diamond.” *Physical Review B* **80** (2009) 125203.

[38] J. Callaway, “Model for lattice thermal conductivity at low temperatures.” *Physical Review*

**113** (1959) 1046.

[39] M. G. Holland, “Analysis of lattice thermal conductivity.” *Physical Review* **132** (1963) 2461.

[40] M. Omini and A. Sparavigna, “Beyond the isotropic assumption in the theory of thermal

conductivity.” *Physical Review B* **53** (1996) 9064–9073.

[41] P. B. Allen and J. L. Feldman, “Thermal conductivity of disordered harmonic solids.” *Physical Review B* **48** (1993) 12581–12588.

[43] D. A. Broido, A.Ward, and N. Mingo, “Lattice thermal conductivity of silicon from empirical

interatomic potentials.” *Physical Review B* **72** (2005) 014308.

[46] W. Frank, C. Els¨asser, and M. F¨ahnle, “Ab initio force-constant method for phonon dispersions

in alkali metals.” *Physical Review Letters* **74** (1995) 1791–1794.

[47] P. Pavone, “Old and new aspects in lattice-dynamical theory.” *Journal of Physics: Condensed*

*Matter* **13** (2001) 7593–7610.